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AUTOMATIC FATALITY PREVENTION AND EMERGENCY AID SYSTEM
https://www.youtube.com/watch?v=FrIEjB9cL18

The main aim of this project is to develop an automatic fatality prevention and Emergency AID system using sensors like ADXL345 MEMS accelerometer, SR04 Ultrasonic sensor, IR Flame sensor for preventing accident and fire detections. The project also aims in tracking of the vehicle using GPS and GSM modules. In case of emergency situations, it sends an automatic SMS alerting message to the authorities. 

Ultrasonic sensor is an echo-based sensor which can transmit the sound waves and receives in an echo by using this we can find the distance of the object and prevent the vehicle to hit the object. MEMS is a Micro electro mechanical sensor which is a highly sensitive sensor and capable of detecting the tilt used for accident detection.  The system consists of cooperative components of MEMS accelerometer sensor, Ultrasonic sensor, IR flame sensor, Arduino microcontroller unit, GPS device and GSM module.  In the event of accident, this wireless device will send to mobile phone as a short message indicating the position of vehicle by GPS system to respective authorities, emergency medical service (EMS) and nearest hospital.  The threshold algorithm and speed of motorcycle are used to determine fall or accident in real-time.  The system also alerts through SMS messages when any fire accidents occurred was detected using IR flame sensor

The system is compact and easy to install under rider seat.  An accelerometer can be used in a car alarm application. Dangerous driving can be detected with an accelerometer. It can be used as a crash recorder of the vehicle movements before, during and after a crash. With signals from an accelerometer, a severe accident can be recognized. The system also alerts when engine gets over heated or any fire accident was detected using IR flame sensor. This project makes use of an onboard Arduino microcontroller, which is commonly termed as micro controller. 

Features:
1) MEMS based user-friendly interfacing

2) SR04 Ultrasonic sensor for obstacle detection
3) Detection of Dangerous driving 

4) IR flame sensor for fire detection
5) Highly Sensitive

6) Location based alerts in the for SMS messages sing GSM

7) Accident detection suing MEMS and fire sensors

8) Audible and visual alerts using LCD and buzzer

9) Implementation of REAL TIME embedded system which involves hardware and software interaction.

The major building blocks of this project are:

1. Regulated power supply with voltage regulator.

2. MEMS accelerometer sensor.

3. GPS module.

4. SR04 Ultrasonic sensor (obstacle detection)
5. IR flame sensor (fire detection)
6. LCD

7. Buzzer

8. Arduino UNO Microcontroller.

9. GSM Modem.
Software’s used:

1. Arduino IDE for compiling and dumping code into Microcontroller
2. Express SCH for Circuit design.

Regulated Power Supply:
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Block Diagram:
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www.hvstechnologies.in                                                                            Ph: +91 9603140482

Ameerpet:      #A-7, 2nd floor, Eureka court, Above KS bakers, Ameerpet, Hyderabad – 73.

Dilsukhnagar: #F-8, 1st floor, Sreemaan Rama Towers, Opp:Kalanikethan, Chaitanyapuri, Hyderabad - 62.
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